%UGII_BASE_DIR%\UGMANAGER\ugmanager_refile_program.exe

Teamcenter Integration Refile Utility  Version: NX 7.5.1.5 (Date 07.11.2010)
	-u[ser]=<user> to specify Teamcenter user name
	-g[roup]=<group> to specify Teamcenter group name
	-p[assword] to specify Teamcenter password
	-pf=<filename> file to specify the Teamcenter password
	-i[nput_list]=<filename> list of specifications of parts to refile
	-f[older]=<foldername> name of folder listing parts to refile
	-k[eep_volume]=<yes|no> use original volume for refiled parts
	-h[elp] produces this message
	-d[rawings] =<update> update drawings
	-non[_masters]=<yes|no> automatically refile non-master parts
	-out[put_file]=<filename> file to write failure information to
	-log[_file]=<filename> file to write log information to
	-part=<part spec> specification of single part to refile
	-bypass=<yes|no> use bypass privilege if necessary
	-resume[_from]=line number of input list to start processing from
	-update_mod[_props]=<yes|no> update last modifying user/date on dataset
	-set_new_dataset_o[wner] sets the ownership of new datasets to be either that of the owning item-rev or multi-CAD jt dataset
	-refile_released=<yes|no> refile parts with release status
	-structure_sync=<no|from_teamcenter|from_ug> synchronize structures during refile
	-force_structure_sync=<yes|no> force synchronize structures during refile as requested by -structure_sync
	-transforms_source=<from_teamcenter|from_ug> source of transforms if different from -structure_sync argument
	-allow_null_transform used with -structure_sync=from_teamcenter and -transforms_source=from_teamcenter to allow transforms from Teamcenter to be null
	-sync_arrangements=<yes|no> synchronize arrangement data if consistent with other structure sync settings
	-read_mapped_attri[butes]=<yes|no> read mapped attributes if consistent with other structure sync settings
	-generate_trueshape=<yes|no> generate True Shape occupancy data without refiling parts
	-record_part_data=<yes|no> record part data (Bounding Box, Mass Properties) without refiling parts
	-record_altrep_notes=<yes|no> record AltRep occurrence notes without refiling parts
	-compression=<compress|uncompress> compresses|uncompresses the part(s) when refiling
	-y fully load assembly and refile components that are not at the current version of NX
	-force_refile used with the -y switch to force all components to be refiled
	-cleanu[p]=<yes|no> perform part cleanup before refiling
	-anon[ymize]=<yes|no> removes user and program version strings from part history
	-force_read_jt force to read from a JT dataset even if a master dataset exists
	-convert_mcs=<filename> convert mating conditions to assembly constraints and output report
	-mc_parts_only used in conjunction with convert_mcs to specify only convert parts which contain mating conditions
	-mc_dry_run used in conjunction with convert_mcs to do the mating condition conversion and generate the conversion report without saving any parts.
	-mc_dont_load_referenced_geometry used in conjunction with convert_mcs to not load geometry referenced by the mating conditions being converted. Note this will bypass constraint conversion checking.
	-regen_lw force all lightweight bodies in the specified part to be regenerated. By default the faceting parameters
       previously used to create each body will be used again. This option is now being done by default for parts saved before NX7.5.

	-regen_lw_use_def[_tol] similar to regen_lw however this flag will not use the faceting parameters on the existing body
       but the default faceting parameters will be utilized instead.

	-remap_drawing_callouts=<attribute_name> remap the callout references in drawing to <attribute_name>
	-synchronize_callout_to_teamcenter=<normal|force_skip_one_level> update the Find No. in Teamcenter based on the CALLOUT value on the NX part occurrences


