Catia V5 <-> NX translator

Copyright 2022 Siemens All Rights Reserved.
This software and related documentation are proprietary to Siemens Industry Software Inc.

Parts of the UG/Knowledge Fusion software have been provided by Heide
Corporation. Copyright (c) 1997 Heide Corporation. All Rights Reserved.

This product includes software developed by the Apache Software
Foundation ( http://www.apache.org/).

This product includes the International Components for Unicode software
provided by International Business Machines Corporation and others.
Copyright (c) 1995-2001 International Business Machines Corporation and
others. All rights reserved.

Portions of this software are copyright (c) 2007 The FreeType Project
(www.freetype.org). All rights reserved.

Portions of this software are copyright (C) 2013 Digia Plc and/or its subsidiary(-ies).
Contact: http://www.qt-project.org/legal.
This product includes modified MUMPS software.
Copyright 1991 - 2017 CERFACS, CNRS, ENS Lyon, INP Toulouse, Inria, University of Bordeaux.

MATLAB(r). (c) 1984-2019 The MathWorks, Inc.

Portions of this software are copyright (c) 2019 Bentley Systems, Incorporated Version 02.06.02.05 PointoolsVortexAPI
Contact ( https://www.bentley.com/). All rights reserved.

For further information on all the third party software included in this release please refer to the Readme_OSS file.


  Initializing... NX2212.6000
No input parts provided. Exiting translator.

Usage: catiav5.exe [I=]myinputfile.<extension>
                   [O=myoutputfile.<extension>]
                   [D=mycatiav5.def]
                   [L=mylogfile.log]
                   [-inch] (import as inches)

       All arguments are optional except for the input file.

       The translator treats all command line arguments without an
       option prefix as either a CATIA V5 input file (extensions
       .CATProduct, .CATPart, .CATShape, and.cgr) or an NX input
       part (extension .prt).

       If you do not specify a d=<settings file>, catiav5.def from
       the installation kit will be used.
